# -------------------------------------------------------------------------- #
#
# Copyright (C) 1991-2013 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files from any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Altera Program License 
# Subscription Agreement, Altera MegaCore Function License 
# Agreement, or other applicable license agreement, including, 
# without limitation, that your use is for the sole purpose of 
# programming logic devices manufactured by Altera and sold by 
# Altera or its authorized distributors.  Please refer to the 
# applicable agreement for further details.
#
# -------------------------------------------------------------------------- #
#
# Quartus II 64-Bit
# Version 13.1.0 Build 162 10/23/2013 SJ Web Edition
# Date created = 03:40:23  July 19, 2020
#
# -------------------------------------------------------------------------- #
#
# Notes:
#
# 1) The default values for assignments are stored in the file:
#		Zadatak2_assignment_defaults.qdf
#    If this file doesn't exist, see file:
#		assignment_defaults.qdf
#
# 2) Altera recommends that you do not modify this file. This
#    file is updated automatically by the Quartus II software
#    and any changes you make may be lost or overwritten.
#
# -------------------------------------------------------------------------- #


set_global_assignment -name FAMILY "Cyclone III"
set_global_assignment -name DEVICE EP3C16F484C6
set_global_assignment -name TOP_LEVEL_ENTITY main4
set_global_assignment -name ORIGINAL_QUARTUS_VERSION 13.1
set_global_assignment -name PROJECT_CREATION_TIME_DATE "03:40:23  JULY 19, 2020"
set_global_assignment -name LAST_QUARTUS_VERSION 13.1
set_global_assignment -name PROJECT_OUTPUT_DIRECTORY output_files
set_global_assignment -name MIN_CORE_JUNCTION_TEMP 0
set_global_assignment -name MAX_CORE_JUNCTION_TEMP 85
set_global_assignment -name ERROR_CHECK_FREQUENCY_DIVISOR 1
set_global_assignment -name NOMINAL_CORE_SUPPLY_VOLTAGE 1.2V
set_global_assignment -name BDF_FILE main1.bdf
set_global_assignment -name BDF_FILE main2.bdf
set_global_assignment -name BDF_FILE main3.bdf
set_global_assignment -name BDF_FILE main4.bdf
set_global_assignment -name PARTITION_NETLIST_TYPE SOURCE -section_id Top
set_global_assignment -name PARTITION_FITTER_PRESERVATION_LEVEL PLACEMENT_AND_ROUTING -section_id Top
set_global_assignment -name PARTITION_COLOR 16764057 -section_id Top
set_global_assignment -name STRATIX_DEVICE_IO_STANDARD "2.5 V"
set_location_assignment PIN_H2 -to BTN0
set_location_assignment PIN_G3 -to BTN1
set_location_assignment PIN_F1 -to BTN2
set_location_assignment PIN_G21 -to clk
set_location_assignment PIN_E11 -to H00
set_location_assignment PIN_F11 -to H01
set_location_assignment PIN_H12 -to H02
set_location_assignment PIN_H13 -to H03
set_location_assignment PIN_G12 -to H04
set_location_assignment PIN_F12 -to H05
set_location_assignment PIN_F13 -to H06
set_location_assignment PIN_A13 -to H10
set_location_assignment PIN_B13 -to H11
set_location_assignment PIN_C13 -to H12
set_location_assignment PIN_A14 -to H13
set_location_assignment PIN_B14 -to H14
set_location_assignment PIN_E14 -to H15
set_location_assignment PIN_A15 -to H16
set_location_assignment PIN_D15 -to H20
set_location_assignment PIN_A16 -to H21
set_location_assignment PIN_B16 -to H22
set_location_assignment PIN_E15 -to H23
set_location_assignment PIN_A17 -to H24
set_location_assignment PIN_B17 -to H25
set_location_assignment PIN_F14 -to H26
set_location_assignment PIN_B1 -to LED[9]
set_location_assignment PIN_B2 -to LED[8]
set_location_assignment PIN_C2 -to LED[7]
set_location_assignment PIN_C1 -to LED[6]
set_location_assignment PIN_E1 -to LED[5]
set_location_assignment PIN_F2 -to LED[4]
set_location_assignment PIN_H1 -to LED[3]
set_location_assignment PIN_J3 -to LED[2]
set_location_assignment PIN_J2 -to LED[1]
set_location_assignment PIN_J1 -to LED[0]
set_location_assignment PIN_D2 -to SW9
set_location_assignment PIN_B18 -to H30
set_location_assignment PIN_F15 -to H31
set_location_assignment PIN_A19 -to H32
set_location_assignment PIN_B19 -to H33
set_location_assignment PIN_C19 -to H34
set_location_assignment PIN_D19 -to H35
set_location_assignment PIN_G15 -to H36
set_instance_assignment -name PARTITION_HIERARCHY root_partition -to | -section_id Top